4.	Revisions and additions proposed to Recommendation M.565

ACCESS POINTS FOR INTERNATIONAL TELEPHONE CIRCUITS

In § 2.1.1 the second sentence of the paragraph following the definition "line access points" has to be changed to read:

"In this case any necessary testing of circuits carried out at ...

(rest unchanged)."

In § 2.1.1 the third sentence of the paragraph following the definition of "line access points" has to be replaced by:

"Circuit tests which involve the sending of test signals should be

carried out from the circuit access point as defined in § 2.1.2 below."

Add the following alinea to § 2.1.2:

"Where a circuit uses channel associated signalling it should be

possible to identify and measure at the circuit access points, the signal-transmission parameters, e.g. type of signal, sequence, timing, duration, level and frequency."