TABLE 1/T.100
Display modes and control characters–serial mode
 Display mode	 Set at	Set after
(see Note)	 Complementary display mode	 Set at	Set after
(see Note)	
 Alphanumerics	 Row start	4/1   4/2   4/3 
4/4   4/5   4/6   4/7	 Block mosaics	 –	 5/1   5/2   5/3
 5/4   5/5   5/6  5/7	
 Contiguous	Row start 5/9	 5/9	 Separated	 5/10	 5/10	
Fore-
ground display colour	 includes  red	 Row start	4/1   4/3   4/5   4/7 
5/1   5/3   5/5   5/7	Fore-
ground display colour	 includes  red	–	4/2   4/4   4/6
5/2   5/4   5/6	
 	 includes green	 Row start	 4/1   4/2   4/3   4/7 
5/1   5/2   5/3   5/7		 excludes green	–	4/1  4/4   4/5 
5/1   5/4  5/5 	
	 includes blue	 Row start	4/4   4/5  4/6  4/7
5/4   5/5   5/6   5/7		 excludes blue	–	4/1  4/2   4/3
5/1   5/2   5/3	
Black background	Row start 5/12	–	New background colour	5/13	 –	

Stop conceal	
Row start	4/1       4/2       4/3
4/4   4/5   4/6   4/7
5/1     5/2        5/3
5/4   5/5   5/6   5/7	
Conceal	
5/8 	
–	
Steady	Row start 4/9	–	Flash	 –	 4/8	
Unboxed	Row start 4/10	4/10	Boxed	 4/11	 4/11	
Normal height	Row start 4/12	–	Double height	 –	 4/13	
Release	Row start	5/15	Hold	 5/14	 –	
						
			Note – All attribute control characters are preceded by Escape ESC.