ANNEX C
(to Recommendation E.506)
Description of a top down procedure
	Let
XT	be the traffic forecast on an aggregated level,
Xi	be the traffic forecast to country i,
T	the estimated standard deviation of the aggregated forecast,
i	the estimated standard deviation of the forecast to country i.
Usually
			XT !Unexpected End of Expression. Xi,	(C–1)
so that it is necessary to find a correction
			[X`i] of [Xi] and [X`T] of [XT]
by minimizing the expression
			Q = a0(XT – XT`)2 + !Unexpected End of Expression. ai(Xi – Xi`)2 	(C–2)
subject to 
			XT` = i Xi` 	(C–3)
where a and [ai] are chosen to be
			a0 =  and ai =    i = 1, 2, . . . 	(C–4)
	The solution of the optimization problem gives the values [X`i]:
			Xi` = Xi – 	(C–5)
	A closer inspection of the data base may result in other expressions for the coefficients [ai], i = 0, 1, . . . On some occasions, it will also be reasonable to use other criteria for finding the corrected forecasting values [X`i]. This is shown in the top down example in Annex D.
	If, on the other hand, the variance of the top forecast XT is fairly small, the following procedure may be chosen:
	The corrections [Xi] are found by minimizing the expression
			Q` = !Unexpected End of Expression. ai (Xi – Xi`)2 	(C–6)
subject to
			XT = !Unexpected End of Expression. Xi` 	(C–7)
	If ai, i = 1, 2, . . . is chosen to be the inverse of the estimated variances, the solution of the optimization problem is given by
			Xi` = Xi –   	(C–8)