TABLE B–1/T.70
State table for calling side
	State
Event			Idle												Waiting				
				0.1				0.2				0.3				1.1				
No.	Local	Protocol 
event	Service
 primitive	Local	Protocol
action	Service
primitive	Final state	Local	Protocol 
action	Service
 primitive	Final state	Local	Protocol 
action	Service
primitive	Final state	Local	Protocol 
action	Service
primitive	Final state	
1.1		R–TCR
(E 1)													0.3	STOP 
T1.1 
(A 1) 
START T0.3 (A 2)	S–TBR
(A 3)		0.3	
1.2		Mont.													0.3	RESTART T1.1 (A 6)	S–TCR
(A 7)		1.1	
1.3		Mont.											Discard
any		0.3	STOPT T1.1 
(A 1)		N–DISC 
req. (A 4) 
T–DISC
 ind. (A 5)	0.1	
1.4		R–TCA
(E 3)											R–TPDU (A 14)		0.3	STOPT T1.1
(A 1)		T–CONN. conf (A 8)	2.1	
1.5		R–TBR 
(E 4)													0.3	STOP T1.1
(A 1)		T–DISC.
 ind. (A 5) 
N–DISC.
 req. (A 4)	0.1	
1.6		R–invalid TPDU
(E 5)													0.3	STOP T1.1
(A 1)		T–DISC. 
ind. (A 5) 
N–DISC.
 req. (A 4)	0.1	
1.7			T–CONN. req.(E 6)			T–CONN. req.(A 10)	0.2													
1.8			N–CONN. conf.(E 7)					START T1.1
(A 12)	S–TCR
(A 7)		1.1									
1.9			N–DISC
 ind. (E 8)							T–DISC
 ind. (A 5)	0.1	STOP T0.3 
(A 13)		T–DISC.
 ind. (A 5)	0.1	STOP T1.1
(A 1)		T–DISC.
 ind. (A 5)	0.1	
1.10			N–RESET ind. (E 9)									STOP T0.3 
(A 13)		N–DISC. rec.(A 4) 
T–DISC.
 ind. (A 5)	0.1	STOP T1.1
(A 1)		T–DISC. ind.(A 5) 
N–DISC.
 req. (A 4)	0.1	
1.11			T–DISC
 req. (E 10)							N–DISC. 
req. (A 4)	0.1	STOP T0.3 
(A 13)		N–DISC.
 req. (A 4)	0.1	STOP T1.1
(A 1)		N–DISC
req. (A 4)	0.1	
1.12	TIME–OUT
(E 11)											STOP T0.3 
(A 13)		N–DISC. 
req. (A 4) 
T–DISC.
 ind. (A 5)	0.1	STOP T1.1
(A 1)		T–DISC.
 ind. (A 5) 
N–DISC. 
req. (A 4)	0.1	
Req.	Request			CONN.	CONNECTION
Ind.	Indication			DISC.	DISCONNECTION
Conf.	Confirmation
TABLE B–2/T.70
State table for called side
	State
Event			Idle												Waiting				
				0.1				0.2				0.3				1.1				
No.	Local	Protocol event	Service primitive	Local	Protocol action	Service primitive	Final state	Local	Protocol action	Service primitive	Final state	Local	Protocol action	Service primitive	Final state	Local	Protocol action	Service primitive	Final state	
2.1		Mont.						STOP T0.2 (A 11)		T–CONN. ind. (A 15)	1.1				0.3					
2.2		Mont.						RE-
START T0.2 
(A 16)	S–TCC (A 17)		0.2		Discard any		0.3					
2.3		R–invalid TDPU (E5)						STOP T0.2 (A 11)	N–DISC. req. (A 4)		0.1		R–TPDU (A 14)		0.3	START T0.3 
(A 2)	S–TBR 
(A 3)		0.3	
2.4			Mont.	START T0.2 (A 9)		N–CONN. resp.
(A 22)	0.2													
2.5			Mont.			N–DISC.
 req. (A 4)	0.1													
2.6			T–CONN. resp.
(E 13)														S–TCA 
(A 24)		2.1	
2.7			N–DISC
 ind.(E 8)					STOP T0.2 (A 11)			0.1	STOP T0.3 (A 13)		T–DISC.
 ind. (A 5)	0.1			T–DISC.
 ind. (A 5)	0.1	
2.8			N–RESET ind.(E 9)					STOP T0.2 (A 11)		N–DISC
 req. (A 4)	0.1	STOP T0.3 (A 13)		T–DISC. 
ind. (A 5) 
N–DISC.
 req. (A 4)	0.1			T–DISC. 
ind. (A 5) 
N–DISC.
 req. (A 4)	0.1	
2.9			T–DISC. 
req. (E 10)									STOP T0.3 (A 13)		N–DISC. 
req. (A 4)	0.1	START 
T0.2
(A 9)	S–TCC 
(A 17)		0.2	
2.10	TIME– OUT
(E 11)							STOP T0.2
(A 11)		N–DISC
 req. (A 4)	0.1	STOP T0.3 (A 13)		T–DISC. ind.(A 5) 
N–DISC.
 req. (A4)	0.1					
Req.	Request			CONN.	CONNECTION
Ind.	Indication			DISC.	DISCONNECTION
Resp.	Response